Profanity Delay (Actions)

The information is relevant for version 2.9.34 and later.

Description of Profanity Delay Actions.

Set video stream

Switching the signal source or file source to the module input.

Parameters

Param1 - input stream type

FILE - file source.

LIVE - signal from the software module.

Param2 - file name, software module name.

Set format conversion

Sets the video conversion mode upon a mismatch of the input signal Aspect Ratio and the module settings.

Parameters

Param1 - conversion mode. Possible values: scale, crop, box, letter.

Param2 - AFD use flag. Possible values: true or false.

Set format

Setting the Aspect Ratio of the output signal of the module.

Parameters

Param1 - Aspect Ratio. Possible values: 4:3 or 16:9.

Set delay

Turns on/off the module depending on the parameter.

Parameters

Param1- controls turning on:

1, on, yes or true - starts the module (enables signal delay by the time equal to the Max Delay value). The delayed signal will appear at the module output after the Max Delay interval.

0, off, no or false - disables the delay. The signal appears at the module output with no delay.

Toggle delay

Switches the current mode to the opposite: on→off or off→on. Allows using one key to turn on/off the module.

Parameters

No parameters.

Add delay

Increases the current delay buffer. Added in version 2.9.27.

Parameters

Param1 - the number of frames to add to the delay buffer.

Add delay start

Starts increasing the current delay buffer. Added in version 2.9.27.

Parameters

Param1 - the number of frames to initially add to the delay buffer

Add delay stop

Stops increasing the current delay buffer. Added in version 2.9.27.

Parameters

No parameters.

Drop delay

Reduces the current delay buffer. Added in version 2.9.27.

Parameters

Param1 - the number of frames to delete from the delay buffer.

Drop delay start

Starts reducing the current delay buffer. Added in version 2.9.27.

Parameters

Param1 - the number of frames to initially delete from the delay buffer.

Drop delay stop

Stops reducing the current delay buffer. Added in version 2.9.27.

Parameters

No parameters.

Clear step

Replacement starts after a period equal to (Max Delay-Clear Step), where duration equals Clear Step.

Parameters

Param1 - sound channel mask. Example: 1/2/6/7.

Clear all

Immediately turns on replacement with duration equal to the Max Delay value. Allows activating the replacement process if the operator missed the right moment.

Parameters

Param1 - sound channel mask. Example: 1/2/6/7.

Clear start

Replacement starts after a period equal to (Max Delay-Clear Step) and is implemented with no time limits until the Clear Stop command arrives.

Parameters

Param1 - sound channel mask. Example: 1/2/6/7.

Clear stop

Replacement stops after a period equal to Max Delay.

Parameters

No parameters.

Set Source

Assigns a signal source for the service. Allows assigning a different module’s output as a signal source.

Parameters

Param1 - string with a new signal source. The string is specified in the format: shm_pal://SERVICE. For example: shm_pal://Capture_1