GPI Board (Actions)

The information is relevant for version 2.9.34 and later.

Description of GPI Board Actions.

Set pin

Sets the output status for the selected pin.

Parameters

Param1 - pin number (starts with 1).

Param2 - new pin status:

0, off or false - disable

1, on or true - enable

other values - no changes

Pulse pin

Sends a pulse of the specified duration to the pin output.

Parameters

Param1-

Trigger Handler

Launches the action handlers (pins) when an input signal is detected.

Parameters

Param1 pin number (starts with 1).

Param2 - new pin status:

0, off or false - disable

1, on or true - enable

other values - no changes

Do Command

Perform a command that is typical for a particular type of hardware.

Parameters

Param1 - command name:

sGPI for Louth decoder

set for Ember+

For Louth decoder (Param1=sGPI)

Param2 - Key

Param3 - ID

Param4 - Segment

Param5 - Title

Param6 - on_air

For Ember+ (Param1=set)

Param2 - Pin number

Param3 - Value

Param4 - not used

Param5 - not used

Param6 - not used