Router Bus (Actions)

The information is relevant for version 2.9.96 and later.

Description of Router Bus Actions.

Set pin

Switching the input signal to a specified output of the matrix switcher.

Parameters

* Param1 - comma-separated list of matrix switcher names (Router Name).

* Param2 - output pin number (starts with 1).

* Param3 - input pin number (starts with 1).

Do effect

Performing a device-dependent operation.

Parameters

* Param1 - comma-separated ist of matrix switcher names (Router Name).

* Param2 - effect number (see your matrix switcher documentation).

* Param3 - effect speed, optional parameter.

* Param4 - effect type, optional parameter.

Set effect param

Sets a specific effect parameter.

Parameters

* Param1 - comma-separated list of matrix switcher names (Router Name).

* Param2 - parameter name:

type

speed

mix

src

* Param3 - effect type, optional parameter.

Enable control

Enables control of a connected hardware device. Added in 2.9.96.

Parameters

No parameters.

Disable control

Disables control of a connected hardware device. Added in 2.9.96.

Parameters

No parameters.