VTR (Actions)

Server	Client
Actions

The information is relevant for version 2.9.34 and later.

Description of VTR Actions.

Seek

Rewinding the tape to a specified position.

Parameters

Param1 - timecode value in the mm:ss[:;]ff or hh:mm:ss[:;]ff format, or the number of frames.

Param2 - optional parameter. Preroll - the time interval for prefetching, which will be subtracted from the value specified in Param1. Possible values: timecode in the mm:ss[:;]ff or hh:mm:ss[:;]ff format, or the number of frames. The default value is 5 seconds.

Play

Playback Start

Parameters

No parameters.

Stop

Stops the current operation.

Parameters

No parameters.