Configuration examples

Installation of SL NEO server and client software, Windows settings, software activation

Install demo version of the SL NEO software

First run, express setup of the client software on the workstation using the Wizard

Tutorials for setting up Windows when you install from scratch and reinstall Windows

Configuring the NTP server in Windows

Server and client software activation procedures

Software update order, save server and client settings

Configuring the server platform

Customize the basic components of the server platform

WEB console for managing server settings. Part 1. Section "Status"

WEB console for managing server settings. Part 2. Sections "I/O Boards", "Storages"

WEB-console control server settings. Part 3. Program Outputs

WEB console for managing server settings. Part 4. Recorders

Setup optional HD SDI/HDMI/IP MultiScreen output

Starting the server, what to look for

Setting up and managing access rights to content and system resources

Guidelines for network security and protecting media servers from malware

Configuring client software

Configuring the Air Manager client application

Customizing different client software configurations on one workstation

File Import

Set up automatic import of media files

Operations with audio tracks when importing media files

Air Playback

Adjusting and normalizing the output level of the audio server

Setting multiformat playback of mixed content

Loudness Normalization in SL NEO servers (Loudness Normalization)

Set up auto-loading playlists

Import playlist from Excel

Setup delayed broadcasting (Time Shift)

Customize the Profanity Delay

Setting up automatic switching to air signals from external lines

Receiving and retransmitting teletext packets

Setting up WSS (Widescreen Signaling)

Control the start of events in one playlist from another playlist

Setup Alarm Clip]

Setup to generate reports of executed on-air events

Change the standard DSP when starting Program Channel service

Notification when a certain playlist event is playing

Recording

Setting up automatic switching of signals to server inputs when recording

Automatic control of the recorder from the executable playlist

Set up automatic recording according to the server's internal schedule

Automatic restart of capture services

Graphic design of programs

Organize graphics layers and automate graphics playback

Creating and editing objects in a graphics editor. Part 1, Part 2, Part 3

Examples of creating titles in the graphics editor

Controls how to turn graphic layers on and off

Generating age markers (Actions)

Forming age restriction markers (Secondary Events)

Setup logo management

Automatically change logos with control from the playlist column

Customize the counter displaying the time remaining to the end of the commercial

Create and edit TV clock

Customize effects and transitions between clips in a playlist

Capture Windows "desktop": Skype, YouTube live

Create squeezeback effect

Customize the "Watch_next_titles"

Setting up "Now in Program"

Create Circle Progress Bar

More graphical layers through controlling PIP objects

Receive and display text from external sources

Hosting and displaying text from external sources ("crawl")

Nested compositions and infobar creation

Receive and display data from weather station

Redundancy: main and standby servers working together

Setup playlist synchronization between the primary and backup servers

Setup synchronous parallel recording on the primary and backup servers

Setup synchronization of the main and backup servers

Reserving IP Playout

Generating and receiving tags, automated insertion of regional ads

Setting up SCTE-104 tag generation

Setting up DTMF tag generation in the server output at the central station

Setting up SCTE-104/35 tags reception to control regional advertising output

Setting up DTMF tag reception to control regional advertising

Setting up the automatic start of regional ads based on matching video fragments

Automatically markup material with markers during recording

Work with transport streams

Setup IP broadcasting to the network via UDP/RTP, use virtual Direct Show

Customize multilingual audio for DVB IP/ASI transport streams

Setting up hidden subtitles in DVB transport streams]

Customize receiving IP UDP/RTP streams, signals from webcams and Internet channels

Demultiplexing DVB-ASI/IP transport streams

Server management, device management

Hotkeys

Customize the GPI option (ADLINK PCI/LPCI-7250 series board)

Customize GPI option (ONTRAK ADU208 external USB module)

Setting up the tape recorder control for tape recording