CII Gateway (Actions)

The information is relevant for version 2.9.34 and later.

Description of CII Gateway Actions.

Additional information.

Create Take Item

Loads a media item to the Gateway interface.

Parameters

Param1 - Target ID to be used for Gateway actions

Param2 - Media Title

Param3 - '@’ separated list of graphics param values (optional)

Update Item

Updating the Param field for the existing Gateway item.

Parameters

Param1 - Target ID

Param2 - Integer position of the Param field in an item

Param3 - String to set the Param field

Play Item

Playout of the Gateway item at the Gateway channel mapped to the actual program channel.

Parameters

Param1 - Target ID

Param2 - Gateway Channel ID

Param3 - Virtual layer number (optional)

Preview Item

Play Gateway item (current Gateway item if no ID provided) on preview playout.

Parameters

Param1 - Optional Target ID

Clear Item

Clear item from all active Gateway channels

Parameters

Param1 - Target ID

Clear Channel

Clear Gateway channel: if no layers are provided, clear all layers.

Parameters

Param1 - Gateway Channel ID

Param2 - Optional virtual layer number

Trigger GPI

Trigger Gateway GPI Pin.

Parameters

Param1 - GPI Pin.