Skylark SL NEO file extensions

File extensions used by the Skylark SL NEO platform applications.

File extension	Description
xrc	Layer configuration file in Router Client
fld	Switch field state file in Router Client
ncp	Project NewsCut file
slg	Graphic composition file
slc	The NewsCut file uploaded from the media base to the file system (CUT clip)
awp	Configuration file for AirManager windows
amc	AirManager application configuration file (MediaConnect, NewsCut).
clf	AirManager playlist file
rlf	AirManager record sheet file
sls	File of the Clock, URL or Local Stream type object dumped from the media base
slt	File of the Text type object dumped from the media base
txt	File of Note type object