EazyMuxer Multiplexer/Demultiplexer

The multiplexer-demultiplexer of transport streams broadcasted through ASI/IP interfaces of SL NEO servers, with an additional Time Shift for TS function.

Launching Several Services

Starting from 2.5.1 version, the option of launching several EasyMuxer at one server is available.

The command line format for launching several apps: C:\Program Files (x86)\SL NEO Media Platform\eazymuxer.exe N, where N is the sequence number of the launched copy.

Example:

eazymuxer.exe 1

eazymuxer.exe 2

eazymuxer.exe 3

Calculating the port number for connecting a random EazyMuxer copy to a web-interface is implemented by the formula: 7801+2*(N-1), where N is the sequence number of the launched copy.